
Thank you for downloading Optec Inc's Pyxis Rotator Control software. Optec relies on your feedback in 
order to deliver a quality product. If you find any problems with our software please report them at the
following url: http://www.optecinc.com/astronomy/report_software_issues.htm


Revision History

*****************************************************************************************************
2.1.4	Aug-2011-JTS		Changed XML settings to parse all numeric values as doubles rather than integers.
				This allows the SkyPAOffset to be set to inrements less than 1 degree.
				Added documentation.
				Improved move command by using Round() method rather than casting to integer when 
					converting target position to an absolute step.

*****************************************************************************************************
2.1.3	July-2011-JTS		Changed Pyxis API to parse firmware version culturally invariantlly 
				to resolve localization issues.

*****************************************************************************************************
2.1.2	July-2011-JTS		Fixed bug that prevented driver from moving to a position between 359 and 360. 

*****************************************************************************************************
2.1.1	Jun-2011-JTS		Driver can now move device to positions at less than 1 degree increments.
				Driver can now report position to less than 1 degree increments.

*****************************************************************************************************				
2.0.2	Mar-2010-JTS  		Fixed HomeOnStart bug so that the value gets pushed to the device.

*****************************************************************************************************
2.0.1	Feb-2010-JTS 

*****************************************************************************************************
2.0.0	Nov-2010-JTS		Rewrote ASCOM Driver using C#.NET
				Rewrote Windows Control Program using C#.NET
				Combined installer for ASCOM driver and Control Program
				Updated programs for the ablilty to Halt devices with supporting firmware
				Fixed bug so that program works regardless of PC localization settings
										
*****************************************************************************************************
1.33	Feb-2009-GLP		Original Liberty Basic program for NON-ASCOM pyxis control

*****************************************************************************************************
1.0.4	??????? -EB		Original ASCOM Driver written in VB.NET by Dr. Eric Benson

*****************************************************************************************************