Hello and welcome to TCF-S driver and Commander Version 6.0.0. This version brings about several major changes that are outlined below. IMPORTANT: You should uninstall your old version before updating to version 6.0.0.
1.	Only one installer. TCF-S Commander now uses an any CPU installer package, eliminating the need to choose between x86 and x64.
2.	Local server driver. The TCF-S driver is now an ASCOM local server driver. This allows any number of ASCOM clients to connect to the TCF-S at the same time.
3.	TCF-S Commander is now an ASCOM client. This allows TCCF-S commander to be connected at the same time as the other ASCOM clients.
4.	An improved Temperature Wizard. The wizard more accurately calculates temperature coefficients. 
5.	TCF-S Commander can now move the focuser during Temperature Compensation. This only applies to the TCF-S Commander program. Other ASCOM clients may not have this capability.
6.	Added Temperature Compensation at Start. This new feature allows focusers that have be recalibrated with the updated temperature wizard to automatically focus at the start of the night. When this mode is active when the TCF-S connects it will compensate for any changes in temperature while it was off and will enter temp comp mode. See the documentation for more details. 
